Has anyone developed a ruleset to test for both the router down or router unreachable conditions?  We have had times when we get router unreachable but no router down and vice versa but do not want to have two different rulesets which would each send a page for different events on the same outage.

Clifford L. Crane - Technical Consultant
Excel Corporation IT Business Continuation
151 N. Main Street
Wichita, KS  67201
Phone (316)291-2899   Fax (316)261-5902
cliff_crane@cargill.com